**Apparel Check List (Children’s)**

**(clothing, wearables, sashes, hat, scarves, mittons)**

**Garment Requirements**

[ ]  Lead in Paints and Surface Coatings. 16 CFR 1303, CPSIA Section 101; (<90ppm)

 [ ]  Test conducted by Accredited Third Party Lab.

[ ]  Testing was conducted within the past 12 months.

*Testing not required if the garment contains no surface coatings/paints.*

[ ]  Total Lead in Substrates. CPSIA Section 101, (<100ppm).

 [ ]  Test conducted by Accredited Third Party Lab.

[ ]  Testing was conducted within the past 12 months.

*Testing not required if the garment is made up of 100% fabric. If the garment contains buttons, rivets, zippers, or other non-fabric elements, testing is required.)*

[ ]  Flame Retardants: PentaBDE, OctaBDE, DecaBDE, TCEP. No detection.

[ ]  Formaldehyde in Children’s Products. MN 325F, Sec. 176-178. No detectable levels.

[ ]  Fiber Content/Analysis AATCC 20/20A

*Testing not required if vendor provides data.*

[ ]  Drawstrings. 16 CFR 1120/ASTM F1816: Neck/hood area: No drawstrings. Waist/Bottom area: may not extend > 3” past channel when garment expanded to fullest width. No toggles/knots at free end. Drawstring must be sewn to garment so it cannot be removed from garment.

*Testing not required. Visual inspection acceptable.*

[ ]  Flammability of wearing apparel. 16 CFR 1610

[ ]  Flammability of vinyl material. 16 CFR1611

 *Testing not required if no vinyl present in garment.*

[ ]  Flammability of Solids. 16 CFR 1500.44

 *Testing not required unless accessories present.*

[ ]  Sharp Points. 16 CFR 1500.48

[ ]  Sharp Points (Metal or Glass). 16 CFR 1500.49

 *Testing not required if no metal or glass.*

[ ]  Small Parts. 16 CFR 1500.50/16 CFR 1501

*Appropriate mechanical hazard testing must be conducted to determine if accessories affixed to the garment are removable from the garment under normal use and wear. No testing required in the case of a simple t-shirt or sweatshirt, for example, that contains no buttons or other fixtures.*

[ ]  Tracking Label. CPSIA 103;

 *Testing not required. Visual inspection is ok.*

* Permanently affixed to product
* Name of Manufacturer
* Location of Manufacture
* Date of Manufacture
* Unique Tracking Number

[ ]  Care Labeling. 16 CFR 423

*Testing not required and a visual inspection is ok provided the vendor provides the information.*

[ ]  Textile Fiber Products Identification/RN#.16 CFR 303/300

 *Testing not required; visual inspection ok.*

[ ]  Country of Origin Marking. 19 CFR 134.11

 *Testing not required; visual inspection ok.*

[ ]  Children’s Product Certificate

[ ]  Recent Test Report (less than 12 months old)

**California Prop 65**

[ ]  Lead in Substrates and Surface Coatings <90 ppm

*May use CPSIA lead testing data. Additional testing typically not required.*

[ ]  Phthalates (DBP, BBP, DEHP, DINP, DIDP, DnHP)

*Testing may not be necessary if no plastic components. Consult with Anseco on a case by case basis.*

[ ]  Total Cadmium in Surface Coatings and Substrates

[ ]  Bisphenol A (BPA) (<100PPT)

***A warning label on the product, packaging and marketing materials will be required for products going into California if phthalates/Cadmium/BPH is in excess of the safe harbor limits. If lead is in excess of the 90/100 ppm, the product may not be sold anywhere in the United States as the product would be deemed a banned hazardous substance.***

**Washington Children’s Safe Products Act 70.240**

*(Applicable to any of the following: toys, children’s cosmetics, children’s jewelry, product used to help a child suck, teeth, sleep, relax, feed, worn as clothing by children, or car seats. Applies to children 12 years of age or younger).*

[ ]  Lead <90ppm in product or product component

[ ]  Cadmium <40ppm in product or product component

[ ]  Phthalates, individually or combined, <1000 ppm in product or product component.

[ ]  Registration if the Children’s Product contains any of the High Priority Chemicals

**Packaging Requirements**

[ ]  TPCH/Coneg/Toxic Elements in Packaging Material (sum of cadmium, hexavalent chromium, lead and mercury in packaging and packaging components shall be < 100ppm by weight)

[ ]  Plastic Bag Warning. **“Warning: To avoid danger of suffocation, keep this plastic bag away from babies and children. Do not use this bag in cribs, beds, carriages or playpens. This bag is not a toy.”**

*Testing not required; visual inspection is ok.*

[ ]  Warning Labels. Likely only required if small parts are present.

 *Testing not required for the evaluation of the warning label language (but testing is required to determine if small parts are present (e.g. zippers, buttons, etc.).*

[ ]  Prop 65 Warning Label if phthalates, cadmium and/or BPA in excess of the safe harbor limits is present.

[ ]  Tracking Label

**Marketing Material Requirements**

[ ]  Warning Labels. Likely only small parts. Must be on all marketing materials (website, catalogs, etc.)

[ ]  Prop 65 Warning Labels (including on websites, catalogs)

Version Control

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Version** | **Description** | **Document #** | **Effective Date** | **Created by:** |
| 1 | Children’s Apparel – Check List | 888792\_1 | 4/29/2016 | Emily Rudie |
| 2 | Apparel Check List (Children’s)* Clothing, wearables, sashes, hats, scarves, mittons added to description
 | 888792\_2 | 07/21/2016 | Emily Rudie |
|  |  |  |  |  |