**Jewelry\* Check List (Children’s)**

**(wristbands, dog tags)**

**Product Requirements**

Lead in Paints and Surface Coatings. 16 CFR 1303, CPSIA Section 101, ASTM F2923-5 (<90ppm)

Test conducted by Accredited Third Party Lab.

Testing was conducted within the past 12 months.

If lead measures between 40ppm – 90 ppm, IL warning required.

*Testing not required if the article contains no surface coatings/paints.*

Total Lead in Substrates. CPSIA Section 101, ASTM F2923.5 (<100ppm).

Test conducted by Accredited Third Party Lab.

Testing was conducted within the past 12 months.

If lead measures between 40ppm – 90 ppm, IL warning required.

Total Lead Content – ASTM F2923-14.

*Testing may not be required if Anseco confirms CPSIA lead test can be used.*

Soluble Heavy Metals in Paint and Surface Coatings. ASTM F2923-14.

Total Cadmium in Substrates. ASTM F2923-14.

Nickel Release. ASTM F2923-14.

Jewelry Mechanical Hazards. ASTM F2923.14.

Jewelry Labeling. ASTM F2923-14.

Flammability of Solids. 16 CFR 1500.44

*Testing not required unless accessories present.*

Formaldehyde in Children’s Products. Minnesota 325F, Sec. 176-178. No detectable levels.

*May not be relevant. Consult with Anseco*

Sharp Points. 16 CFR 1500.48

*Testing may not be required if Anseco advises that the Mechanical tests for ASTM F2923-14 may be relied upon*

Sharp Points (Metal or Glass). 16 CFR 1500.49

*Testing may not be required if Anseco advises that the Mechanical tests for ASTM F2923-14 may be relied upon*.

Tracking Label. CPSIA 103;

*Testing not required. Visual inspection is ok.*

* Permanently affixed to product
* Name of Manufacturer
* Location of Manufacture
* Date of Manufacture
* Unique Tracking Number

Country of Origin Marking. 19 CFR 134.11

*Testing not required; visual inspection ok.*

Children’s Product Certificate

Recent Test Report (less than 12 months old)

Washington Children’s Safe Product Act Total Cadmium in Surface Coatings and Substrates.

Washington Children’s Safe Product Act Phthalate Content (DEHP, DBP, BBP, DINP, DIDP, DnOP)

Warning Labels. Small parts, magnets, etc.

**California Prop 65**

Lead in Substrates and Surface Coatings <90 ppm

*May use CPSIA lead testing data. Additional testing typically not required.*

Phthalates (DBP, BBP, DEHP, DINP, DIDP, DnHP)

*Testing may not be necessary if no plastic components. Consult with Anseco on a case by case basis.*

Total Cadmium in Surface Coatings and Substrates

Bisphenol A (BPA) (<100PPT)

***A warning label on the product, packaging and marketing materials will be required for products going into California if phthalates/Cadmium/BPH is in excess of the safe harbor limits. If lead is in excess of the 90/100 ppm, the product may not be sold anywhere in the United States as the product would be deemed a banned hazardous substance.***

**Washington Children’s Safe Products Act 70.240**

*(Applicable to any of the following: toys, children’s cosmetics, children’s jewelry, product used to help a child suck, teeth, sleep, relax, feed, worn as clothing by children, or car seats. Applies to children 12 years of age or younger).*

Lead <90ppm in product or product component

Cadmium <40ppm in product or product component

Phthalates, individually or combined, <1000 ppm in product or product component.

Registration if the Children’s Product contains any of the High Priority Chemicals

**Packaging Requirements**

TPCH/Coneg/Toxic Elements in Packaging Material (sum of cadmium, hexavalent chromium, lead and mercury in packaging and packaging components shall be < 100ppm by weight)

Plastic Bag Warning. **“Warning: To avoid danger of suffocation, keep this plastic bag away from babies and children. Do not use this bag in cribs, beds, carriages or playpens. This bag is not a toy.”**

*Testing not required; visual inspection is ok.*

Warning Labels. Small parts, magnets, etc.

*Testing not required, visual inspection ok.*

Prop 65 Warning Label if phthalates, cadmium and/or BPA in excess of the safe harbor limits is present.

*Testing not required; visual inspection is ok.*

Tracking Label

*Testing not required; visual inspection is ok.*

Jewelry Label Claims. 16 CFR 23 (i.e. silver vs. silver plated; gold vs. gold colored.)

Age Labeling of Children’s Jewelry. ASTM F2923-4. “Jewelry is not recommended for children under 3 except under close parental supervision.”

Country of Origin

**Marketing Material Requirements**

Warning Labels. If applicable, must be on all marketing materials (website, catalogs, etc.)

Prop 65 Warning Labels (including on websites, catalogs)

Jewelry Label Claims. 16 CFR 23 (i.e. silver vs. silver plated; gold vs. gold colored.)

Age Labeling of Children’s Jewelry. ASTM F2923-4. “Jewelry is not recommended for children under 3 except under close parental supervision.”

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Version** | **Description** | **Document #** | **Effective Date** | **Created by:** |
| 1 | Children’s Jewelry – Checklist | 889839\_1 | 4/29/2016 | Emily Rudie |
| 2 | Jewelry Check List (Children’s)   * Country of Origin added | 889839\_2 | 07/20/2016 | Emily Rudie |
| 3 | Jewelry Check List (Children’s)   * Wristbands added * Dog Tags added | 889839\_3 | 07/21/2016 | Emily Rudie |